<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<packages>
<package name="SOIC8">
<description>&lt;b&gt;SOIC-8&lt;/b&gt; CASE 751-07&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC34164-D.PDF&lt;p&gt;
&lt;b&gt;D (R-PDSO-G8)&lt;/b&gt;PLATIC SMALL-OUTLINE PACKAGE&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/tlc27l2.pdf</description>
</package>
</packages>
<symbols>
<symbol name="P82B96">
<pin name="SX"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SY"/>
<pin name="RY"/>
<pin name="TY"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="P82B96">
<description>P82B96 
- I2C buffer</description>
<gates>
<gate name="G$1" symbol="P82B96"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RX" pad="2"/>
<connect gate="G$1" pin="RY" pad="6"/>
<connect gate="G$1" pin="SX" pad="1"/>
<connect gate="G$1" pin="SY" pad="7"/>
<connect gate="G$1" pin="TX" pad="3"/>
<connect gate="G$1" pin="TY" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
